Copyright (c) 2002 Xilinx, Inc.  All rights reserved.

Everything in this directory is unsupported.Use at your own risk.

This code represents examples of applications created to run as processes controlled by the Xilinx Micro Kernel (XMK).
The C code examples, and the Makefiles are customized to run on a specific hardware and software platform, and they may have to be modified to run on your hardware/software platform. Some examples require specific hardware and/or software components to be present in the hardware/software platform. See the code for more details.

The Makefile has to be customized to select the right compiler, assembler, archiver and other tools, and to find the include files and libraries needed.

The file out.mfs is a data file that contains an image of an MFS file system for testing.

The xmd.ini file and test.cmd file are used to download the executables and data onto the board using xmd. The typical sequence of commands executed from a xygwin shell is:
xmd (at the xygwin prompt)
source test.cmd (at the xmd prompt)
con (at the xmd prompt)
