FLOWTYPE = CONFIG;
###############################################################
## Filename: bitgen.opt
##
## Option File For Xilinx FPGA Bitgen Flow
## 
## Version: 4.1.1
###############################################################
#
# Options for bitgen (Virtex)
#
# Type "bitgen -h <arch>" for a detailed list of command line options
#
Program bitgen
<inputdir><design>.ncd;   # Input ncd file
#-l;                       # Create logic allocation file
-w;                       # Overwrite existing output file
#-m;                       # Create mask file  
#-g StartUpClk:JTAGCLK;    # for JTAG mode
#-g M1Pin:PULLDOWN;
-f bitgen.ut;
##-bd download.elf;	  # Block RAM data file
# Enable only for 4K devices
#-g ReadCapture:Enable;    # Enable ReadCapture 
END Program bitgen
